#N canvas 10 40 620 460 12;
#X text 223 149 <-- click here \,;
#X obj 8 10 cnv 15 400 40 empty empty outlet_order 20 12 0 24 -228992
-66577 0;
#X msg 153 149 3 2 1;
#X obj 101 234 print último;
#X obj 388 234 print first;
#X obj 240 234 print nächste;
#X text 19 374 There are occasional exceptions where it makes sense
to break this convention. But you shouldn't do it unless it really
is necessary. This will save you in the long run.;
#X text 15 80 Just like the flow of programming in Pd \, the data should
be output from right to left.;
#N canvas 10 40 620 460 spread 0;
#X obj 68 2 inlet;
#X obj 38 235 outlet;
#X obj 201 235 outlet;
#X obj 345 235 outlet;
#X obj 66 109 unpack float float float;
#X connect 0 0 4 0;
#X connect 4 0 1 0;
#X connect 4 1 2 0;
#X connect 4 2 3 0;
#X restore 153 188 pd spread the love;
#X text 18 310 While there is nothing forcing you to output data to
the outlets in any order \, Pd has a very strong convention for how
data should be output from an object.;
#X text 175 259 now check the Pd window;
#X connect 2 0 8 0;
#X connect 8 0 3 0;
#X connect 8 1 5 0;
#X connect 8 2 4 0;
