#N canvas 251 9 495 634 10;
#N canvas 240 135 476 472 other_midi_objects 0;
#X obj 55 31 ctlin;
#X obj 97 31 pgmin;
#X obj 140 30 bendin;
#X obj 191 29 touchin;
#X obj 252 29 polytouchin;
#X obj 337 29 midiin;
#X obj 388 28 sysexin;
#X obj 6 85 noteout;
#X obj 63 84 ctlout;
#X obj 161 85 touchout;
#X obj 225 84 polytouchout;
#X obj 314 84 midiout;
#X obj 113 84 pgmout;
#X obj 11 153 makenote;
#X text 10 194 MIDI notes deconstruction:;
#X text 8 128 MIDI note construction:;
#X text 8 58 MIDI output:;
#X text 8 2 MIDI input:;
#X obj 15 226 stripnote;
#X text 11 266 Additional useful objects for MIDI processing (Maxlib
by Olaf Matthes);
#X obj 148 297 chord;
#X obj 109 296 borax;
#X obj 54 296 score o;
#X obj 13 296 pitch;
#X text 15 336 Also \, from cyclone (alpha) by Krzysztof Czaja:;
#X obj 16 359 midiformat;
#X obj 172 359 midiflush;
#X obj 98 359 midiparse;
#X text 15 386 and xeq \, from the same developer;
#X obj 16 411 xeq;
#X text 41 402 an experimental MIDI sequencer;
#X obj 8 31 midiin;
#X restore 89 430 pd other_midi_objects;
#X obj 285 469 pddp/pddplink all_about_midi_flags.pd -text all_about_midi_flags;
#X text 21 469 for an explanation of MIDI usage in Pd see:;
#X obj 18 16 ctlout;
#X text 14 43 The [ctlout] objects sends control messages to the MIDI
port. See a MIDI specification chart for various controller numbers/values
descriptions.;
#X text 15 89 Arguments (optional):;
#X text 24 105 1st (or only one) argument represents the controller
number to transmit to.;
#X text 24 137 2nd argument designates the channel number to transmit
on. If no channel is specified it transmits on channel 1;
#X floatatom 21 181 5 0 0;
#X obj 21 231 ctlout;
#X floatatom 39 197 5 0 0;
#X floatatom 57 213 5 0 0;
#X text 108 175 Inlets:;
#X text 107 240 Outlets: none. Transmits directly to the MIDI port.
;
#X text 120 192 Left: (int) control value (0-127).;
#X text 120 207 Middle: (int) controller number.;
#X text 120 223 Right: (int) channel number.;
#X text 21 264 NOTE: the left inlet accepts also a list of (2 or 3)
integers where the first item is controller value \, second controller
number and third the channel number.;
#X obj 24 356 ctlout;
#X obj 116 356 ctlout 64;
#X obj 218 356 ctlout 64 2;
#X obj 320 355 ctlout;
#X msg 43 337 64;
#X msg 73 337 2;
#X msg 317 320 67 64 2;
#X floatatom 218 318 5 0 0;
#X floatatom 116 316 5 0 0;
#X floatatom 24 316 5 0 0;
#X msg 173 333 2;
#X text 23 379 All these examples will transmit control no 64 on channel
2 (remember to click the message boxes to initialize).;
#X text 22 411 See also:;
#X obj 25 430 ctlin;
#X text 66 17 - send MIDI control messages to the MIDI port;
#X text 19 515 This document was updated for Pd version 0.35 by Michal
Seta as part of a project called pddp proposed by Krzysztof Czaja \,
managed and edited by Dave Sabine \, to build comprehensive documentation
for Pd.;
#X connect 8 0 9 0;
#X connect 10 0 9 1;
#X connect 11 0 9 2;
#X connect 22 0 18 1;
#X connect 23 0 18 2;
#X connect 24 0 21 0;
#X connect 25 0 20 0;
#X connect 26 0 19 0;
#X connect 27 0 18 0;
#X connect 28 0 19 2;
