#N canvas 10 40 620 460 12;
#X obj 99 238 +;
#X floatatom 99 267 5 0 0 0 - - -;
#X msg 99 184 1;
#X msg 117 215 5;
#X text 11 54 For most objects in Pd \, the leftmost inlet is the "hot"
inlet. This means that it will output something whenever it receives
data on the "hot" inlet.;
#X text 145 215 2) click this and there will be no new output;
#X obj 181 350 +;
#X floatatom 181 374 5 0 0 0 - - -;
#X msg 84 315 1;
#X text 15 291 Try a number of different combinations to see for yourself:
;
#X text 215 343 <-- "cold" inlet;
#X text 49 343 "hot" inlet -->;
#X msg 124 315 2;
#X msg 164 315 3;
#X msg 234 315 4;
#X msg 274 315 5;
#X msg 314 315 6;
#X text 145 184 1) click this first \, and [+ ] immediately outputs
a 1;
#X obj 6 8 cnv 15 400 40 empty empty hot_and_cold_inlets 20 12 0 24
-228992 -66577 0;
#X text 10 111 All other inlets are generally "cold" inlets \, which
just store the data. When the object receives input on the "hot" inlet
\, the object with read the data from all the inlets and do its thing.
;
#X text 145 242 3) now click the [1( message box;
#X obj 516 97 +;
#X msg 534 73 1;
#X msg 502 73 1;
#X text 17 395 Notice that the number is stored in the "cold" inlet
until you change it. For example \, if you click [4( \, then click
[1( \, [2( \, and [3( \, you will see that 1 \, 2 \, and 3 are all
added to 4;
#X floatatom 516 120 5 0 0 0 - - -;
#X obj 516 140 bng 15 250 50 0 empty empty empty 0 -6 0 10 -262144
-1 -1;
#X connect 0 0 1 0;
#X connect 2 0 0 0;
#X connect 3 0 0 1;
#X connect 6 0 7 0;
#X connect 8 0 6 0;
#X connect 12 0 6 0;
#X connect 13 0 6 0;
#X connect 14 0 6 1;
#X connect 15 0 6 1;
#X connect 16 0 6 1;
#X connect 21 0 25 0;
#X connect 22 0 21 1;
#X connect 23 0 21 0;
#X connect 25 0 26 0;
