#N canvas 322 381 874 375 10;
#X obj 103 77 inlet;
#X obj 161 77 inlet;
#X obj 66 116 f;
#X obj 161 108 select 0;
#X text 323 49 When a new note arrives \, we have to send a Zero to
the velocity outlet together with the last not we got. Immediatly following
that we need to send the new note with the new velocity and store the
new note for the next onset.;
#X connect 0 0 2 1;
#X connect 1 0 3 0;
