#N canvas 293 25 488 486 10;
#X obj 19 12 pgmout;
#X obj 19 134 pgmout;
#X floatatom 19 100 5 0 0;
#X floatatom 55 116 5 0 0;
#X text 93 96 Inlets:;
#X text 105 113 Left: int \, program change value;
#X text 105 135 Right: int \, MIDI channel to send the program change
message on.;
#X obj 25 233 pgmout 2;
#X text 30 289 See also:;
#N canvas 240 135 476 472 other_midi_objects 0;
#X obj 7 29 ctlin;
#X obj 49 29 pgmin;
#X obj 92 28 bendin;
#X obj 143 27 touchin;
#X obj 204 27 polytouchin;
#X obj 289 27 midiin;
#X obj 340 26 sysexin;
#X obj 6 85 noteout;
#X obj 63 84 ctlout;
#X obj 160 84 bendout;
#X obj 217 83 touchout;
#X obj 281 82 polytouchout;
#X obj 370 82 midiout;
#X obj 113 84 pgmout;
#X obj 11 153 makenote;
#X text 10 194 MIDI notes deconstruction:;
#X text 8 128 MIDI note construction:;
#X text 8 58 MIDI output:;
#X text 8 2 MIDI input:;
#X obj 15 226 stripnote;
#X text 11 266 Additional useful objects for MIDI processing (Maxlib
by Olaf Matthes);
#X obj 148 297 chord;
#X obj 109 296 borax;
#X obj 54 296 score o;
#X obj 13 296 pitch;
#X text 15 336 Also \, from cyclone (alpha) by Krzysztof Czaja:;
#X obj 16 359 midiformat;
#X obj 172 359 midiflush;
#X obj 98 359 midiparse;
#X text 15 386 and xeq \, from the same developer;
#X obj 16 411 xeq;
#X text 41 402 an experimental MIDI sequencer;
#X restore 109 316 pd other_midi_objects;
#X obj 295 354 pddp/pddplink all_about_midi_flags.pd -text all_about_midi_flags;
#X text 25 353 for an explanation of MIDI usage in Pd see:;
#X text 92 166 Outlets: None. Sends directly to the MIDI port;
#X floatatom 25 205 5 0 0;
#X obj 31 316 pgmin;
#X text 16 40 Arguments: (optional) and int representing the MIDI channel
to which the program change should be sent. Without an argument it
will send on channel 1 by default.;
#X text 24 262 Send program change message on MIDI channel 2;
#X floatatom 193 205 5 0 0;
#X msg 238 204 2;
#X obj 193 233 pgmout;
#X text 70 12 - send program change messages to the MIDI port;
#X text 23 393 This document was updated for Pd version 0.35 by Michal
Seta as part of a project called pddp proposed by Krzysztof Czaja \,
managed and edited by Dave Sabine \, to build comprehensive documentation
for Pd.;
#X connect 2 0 1 0;
#X connect 3 0 1 1;
#X connect 13 0 7 0;
#X connect 17 0 19 0;
#X connect 18 0 19 1;
