#N canvas 244 81 496 558 10;
#X text 118 123 outlets:;
#X floatatom 16 149 5 0 0 0 - - -;
#X floatatom 59 149 5 0 0 0 - - -;
#N canvas 240 135 476 472 other_midi_objects 0;
#X obj 7 29 ctlin;
#X obj 49 29 pgmin;
#X obj 92 28 bendin;
#X obj 143 27 touchin;
#X obj 204 27 polytouchin;
#X obj 289 27 midiin;
#X obj 340 26 sysexin;
#X obj 6 85 noteout;
#X obj 63 84 ctlout;
#X obj 160 84 bendout;
#X obj 217 83 touchout;
#X obj 281 82 polytouchout;
#X obj 370 82 midiout;
#X obj 113 84 pgmout;
#X obj 11 153 makenote;
#X text 10 194 MIDI notes deconstruction:;
#X text 8 128 MIDI note construction:;
#X text 8 58 MIDI output:;
#X text 8 2 MIDI input:;
#X obj 15 226 stripnote;
#X text 11 266 Additional useful objects for MIDI processing (Maxlib
by Olaf Matthes);
#X obj 148 297 chord;
#X obj 109 296 borax;
#X obj 54 296 score o;
#X obj 13 296 pitch;
#X text 15 336 Also \, from cyclone (alpha) by Krzysztof Czaja:;
#X obj 16 359 midiformat;
#X obj 172 359 midiflush;
#X obj 98 359 midiparse;
#X text 15 386 and xeq \, from the same developer;
#X obj 16 411 xeq;
#X text 41 402 an experimental MIDI sequencer;
#X restore 20 401 pd other_midi_objects;
#X text 18 346 related object;
#X obj 104 447 pddp/pddplink all_about_midi_flags.pd -text all_about_midi_flags;
#X text 18 421 for an explanation of MIDI usage in Pd see:;
#X obj 33 18 bendin;
#X text 119 103 inlets : none (reads directly from the MIDI port);
#X obj 23 107 bendin;
#X text 9 49 The [bendin] object reads incoming pitch bend values and
reports them. If started with no arguments it reports the channel number
through the right outlet.;
#X text 14 192 Arguments: the MIDI channel number from which to read.
If the argument is present \, the [bendin] object does not show the
second (right) outlet:;
#X obj 25 256 bendin 2;
#X floatatom 25 278 5 0 0 0 - - -;
#X obj 21 361 bendout;
#X text 76 279 <-- pitch bend values on channel 2;
#X text 16 312 Output (int) is a 14-bit pitchbend value;
#X text 130 142 left: pitchbend value;
#X text 129 159 right: MIDI channel number (if no argument);
#X text 81 19 - read incoming pitch bend values.;
#X text 19 482 This document was updated for Pd version 0.35 by Michal
Seta as part of a project called pddp proposed by Krzysztof Czaja \,
managed and edited by Dave Sabine \, to build comprehensive documentation
for Pd.;
#X connect 9 0 1 0;
#X connect 9 1 2 0;
#X connect 12 0 13 0;
